**נספח ו'**

נספח א' – נספח טכני

1. הלקוח יתחבר בפרוטוקול SMPP ו/או HTTPS וישלח הודעות למספרים סלולריים / נייחים.

2. ההודעות שיישלחו במסגרת השירות הן טקסטואליות בלבד.

3. הקצב לשנייה (TPS) שיוקצה ללקוח הוא עד TPS20.

4. אורכי ההודעות ב SMMP לפי התיאור הבא:

The maximum limit of characters per one single submit\_sm depends on the encoding:

160 characters for 7-bit encodings (e.g. ASCII, GSM7bit)

140 characters for 8-bit encodings (Binary, Latin-1)

70 characters for 16-bit encodings (Unicode/UCS-2)

The maximum limit of characters per one submit\_sm of concatenated/long message depends on the encoding:

153 characters for 7-bit encodings (e.g. ASCII, GSM7bit)

134 characters for 8-bit encodings (Binary, Latin-1)

67 characters for 16-bit encodings (Unicode/UCS-2)

Note: Each character from GSM7bit extended alphabet ( ^{}\[~]|€ ) encoded by 14 bits (2 bytes in sm\_text of submit\_sm) and using of them changes total chars limit.

Limits for text in bytes do not change:

up to 140 bytes of text for single sms;

up to 134 bytes of text for concat sms (part of long message).